**How to write the program**

1. After finishing the installation of the device, you are ready to write your first haply program. When testing with your device, make sure the switch on the encoder (the chip at the back of the motor) is on the left side, so the handle on the screen will be able to move when you move the handle.
2. Go to <https://github.com/haphub/WHC2017> and download the folder.
3. Unzip the folder and go to hAPI, we will use the Template\_Sketch inside.
4. Open Template\_Sketch.pde.